[PRN_E1H]
MEANING="CR PID overload error"
DESCRIPTION="- CR Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- CR Motor failure\r\n- Carriage overload error (paper jam/foreign object)\r\n- Cable disconnection"

[PRN_E2H]
MEANING="CR PID over speed error"
DESCRIPTION="- CR Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- Motor driver failure (Main Board failure)\r\n- Tooth skip of the CR Timing Belt\r\n- Improper tension of the CR Timing Belt"

[PRN_E3H]
MEANING="CR PID reverse error"
DESCRIPTION="- CR Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- Tooth skip of the CR Timing Belt\r\n- Improper tension of the CR Timing Belt\r\n- Carriage overload error (paper jam/foreign object)"

[PRN_E4H]
MEANING="CR PID lock error"
DESCRIPTION="- CR Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- CR Motor failure\r\n- Carriage overload error (paper jam/foreign object)\r\n- Cable disconnection"

[PRN_E8H]
MEANING="CR load position control reverse detection error"
DESCRIPTION="- CR Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- Tooth skip of the CR Timing Belt\r\n- Improper tension of the CR Timing Belt\r\n- Carriage overload error (paper jam/foreign object)"

[PRN_E9H]
MEANING="CR load position control over-speed error"
DESCRIPTION="- CR Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- Motor driver failure (Main Board failure)\r\n- Tooth skip of the CR Timing Belt\r\n- Improper tension of the CR Timing Belt"

[PRN_EAH]
MEANING="CR load position control over-load error"
DESCRIPTION="- CR Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- CR Motor failure\r\n- Carriage overload error (paper jam/foreign object)\r\n- Cable disconnection"

[PRN_F1H]
MEANING="PF PID over-load error"
DESCRIPTION="- PF Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- PF Motor failure\r\n- PF drive mechanism overload (paper jam/foreign object)\r\n- Cable disconnection"

[PRN_F2H]
MEANING="PF PID over-speed error"
DESCRIPTION="- PF Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- Motor driver failure (Main Board failure)\r\n- Tooth skip of the PF Timing Belt\r\n- Improper tension of the PF Timing Belt"

[PRN_F3H]
MEANING="PF PID reverse error"
DESCRIPTION="- PF Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- Tooth skip of the PF Timing Belt\r\n- Improper tension of the PF Timing Belt\r\n- Paper jam"

[PRN_F4H]
MEANING="PF PID lock error"
DESCRIPTION="- PF Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- PF Motor failure\r\n- PF drive mechanism overload (paper jam/foreign object)\r\n- Cable disconnection"

[PRN_F8H]
MEANING="PF load position control reverse detection error"
DESCRIPTION="- PF Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- Tooth skip of the PF Timing Belt\r\n- Improper tension of the PF Timing Belt"

[PRN_F9H]
MEANING="PF load position control over-speed error"
DESCRIPTION="- PF Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- Motor driver failure (Main Board failure)\r\n- Tooth skip of the PF Timing Belt\r\n- Improper tension of the PF Timing Belt"

[PRN_FAH]
MEANING="PF load position control over-load error"
DESCRIPTION="- PF Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- PF Motor failure\r\n- PF drive mechanism overload (paper jam/foreign object)\r\n- Cable disconnection"

[PRN_FCH]
MEANING="PF load position target position over decision error"
DESCRIPTION="- PF Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- PF Motor failure\r\n- PF drive mechanism overload (paper jam/foreign object)\r\n- Cable disconnection"

[PRN_EEH]
MEANING="CR(PID) over-driving-time error"
DESCRIPTION="- Main Board failure"

[PRN_EFH]
MEANING="CR(load position control) over-driving-time error"
DESCRIPTION="- Main Board failure"

[PRN_FEH]
MEANING="PF(PID) over-driving-time error"
DESCRIPTION="- Main Board failure"

[PRN_FFH]
MEANING="PF(BS) over-driving-time error"
DESCRIPTION="- Main Board failure"

[PRN_9BH]
MEANING="Transistor environment temp. abnormal error"
DESCRIPTION="- Main Board failure"

[PRN_9CH]
MEANING="Before printing X-hot detection error"
DESCRIPTION="- Printhead failure\r\n- Main Board failure"

[PRN_9DH]
MEANING="After flushing X-hot detection error"
DESCRIPTION="- Printhead failure\r\n- Main Board failure"

[PRN_9EH]
MEANING="Head environment temperature error"
DESCRIPTION="- Printhead failure\r\n- Main Board failure"

[PRN_60H]
MEANING="Home-seek error"
DESCRIPTION="- Carriage overload error (paper jam/foreign object)\r\n- Deformation of the Main Frame\r\n- Ink system failure\r\n- CR Motor failure\r\n- Deformation of the CR Guide Rail\r\n- CR Encoder failure (contaminated/detached scale, Encoder Board failure)\r\n- Cable disconnection"

[PRN_63H]
MEANING="Hit error during ink exchange (Power-off)"
DESCRIPTION="- Paper jam\r\n- Foreign object\r\n- Deformation of the Main Frame"

[PRN_64H]
MEANING="Paper-jam cancelation disable error"
DESCRIPTION="- Paper jam(foreign object)"

[PRN_B9H]
MEANING="Other Ink device error"
DESCRIPTION="- Holder Board Assy failure (CSIC Terminal failure/CR Contact Module failure)\r\n- Main Board failure\r\n- Cable disconnection"

[PRN_BAH]
MEANING="Other Ink device error"
DESCRIPTION="- Holder Board Assy failure (CSIC Terminal failure/CR Contact Module failure)\r\n- Main Board failure\r\n- Cable disconnection"

[PRN_C0H]
MEANING="CRCM access error"
DESCRIPTION="- Holder Board Assy failure (CSIC Terminal failure/CR Contact Module failure)\r\n- Main Board failure\r\n- Cable disconnection"

[PRN_C1H]
MEANING="CRCM access error"
DESCRIPTION="- Holder Board Assy failure (CSIC Terminal failure/CR Contact Module failure)\r\n- Main Board failure\r\n- Cable disconnection"

[PRN_C3H]
MEANING="Other Ink device error"
DESCRIPTION="- Holder Board Assy failure (CSIC Terminal failure/CR Contact Module failure)\r\n- Main Board failure\r\n- Cable disconnection"

[PRN_9AH]
MEANING="Fuse break and circuit error"
DESCRIPTION="- Main Board failure"

[SCN_10H]
MEANING="HP detection failure"
DESCRIPTION="- CIS Unit failure\r\n- Scanner Housing failure\r\n- Main Board failure\r\n- Insufficient grease\r\n- Foreign object\r\n- FFC for CIS failure / FFC for CIS connection failure"

[SCN_20H]
MEANING="LED light failure"
DESCRIPTION="- CIS Unit failure\r\n- Main Board failure"

[SCN_14H]
MEANING="Measurement error"
DESCRIPTION="- Scanner drive mechanism was overloaded"

